Module 4 Asterisk commands

raspbx login -- root

passwd -- beaglebone

cd /etc/asterisk

mv extensions.conf extensions.sample

nano extensions.conf

[from-external]

exten = 100,1,Answer()

same = n,Wait(1)

same = n,Playback(hello-world)

same = n,Hangup()

mv sip.conf sip.backup

nano sip.conf

[general]

context=default

[6001]

type=friend

context=from-external

host=dynamic

secret=unsecurepassword

disallow=all

allow=ulaw

asterisk -rx "core restart now"

asterisk -rvvvvv